**SECTION 504 ARCHITECTURAL PROJECTIONS INTO REQUIRED YARDS**

 All architectural projections shall be in accordance with the following provisions:

 504.1 Chimneys, flues, sills, pilasters, cornices, eaves, gutters, and other similar architectural features may project into any required minimum yard a maximum of 24 inches.

 504.2 Unroofed porches and steps may extend from the dwelling into the required front yard a maximum of 10 feet. Open structures such as roofed porches, canopies, balconies, decks, platforms, and carports, shall be considered parts of the building to which attached and shall not project into any minimum required yard.

NOTE: The entirety of Section 504 is replaced by the above text.